LED mode Requires /LED or command line parameter; Disables built-in spectrum analyzer control. Uses NumLock, CapsLock, Scrolllock LED for spectrum or other information For special state information, the first LED (NumLock) is OFF:

|  |  | stopped
|  |  | paused
|  |  | refreshing
|  |  | deleting file(s)
|  |  | Either caused by a full spectrum, or startup/quitting/output mode change
|  |  | Empty playlist and/or delayed autorefresh

| ( |  | = off, |  | = on, |  | = blinking)

If you operate Calaym without a monitor, the Delayed AutoRefresh feature may be handy when switching discs.